There may be two sources of water: (1) surface, or (2) ground. Each are treated differently.

The main components defining the energy use are:

1. The energy source for the pumping/moving of water (diesel, electricity, solar, etc.)
2. If ground water, the pump pressure and pump depth
3. The amount of irrigation water applied

For liquid fuels, the energy source is converted to BTUs per gallon of fuel.

For electricity, unless the electricity is produced on-farm, the amount of electricity is multiplied by an on-grid factor (3, accounts for Production and transmission loss, FTM calculation from USDOE data, seems insanely high to me). The kilowatt-hours are converted to BTUs.

To get the amount of energy needed to move the water, engineering things are used.

Convert the pumping pressure and pumping depth to meters. Sum them together to get the total pumping head.

The head times the conversion factor (no idea where this comes from; 0.0979) times the amount of water applied (in mm? why in mm?) times the area of the field. This is divided by the ‘efficiency factors’ which I don’t follow.

**Examples:**

**Option #1 Example:** User selects "Diesel fuel" as energy source and inputs 30 gallons for fuel amount used on his or her 4-acre field yielding 220 bu/acre irrigated and 140 bu/acre when not.

Irrigation Energy (**IE**) = (30 gallons x 138,490 BTU/gal) / 4 acres) = 1,038,675 BTU/acre

**Option #2 Example:** User selects "Electricity – Grid" as energy source and inputs 1000 kWh/yr for the Electric amount used on his or her 4-acre field yielding 220 bu/acre when irrigated and 140 bu/acre when not.

Irrigation Energy (**IE**) = (1,000 kWh x 3 x 3414) / 4 acres) = 2,560,500 BTU/acre

**Option #3 Example:** User selects "Electricity – Grid" as energy source. The grower knows he or she made 220 bu/acre (corn) and applied 8.6 ac-in of irrigation water with a pump pressure of 55 psi and pumping depth of 200 ft. If the field were not irrigated the farmer would have grown 140 bu/acre corn. The grower does not know how much electricity was consumed by irrigating his or her 225-acre field. How much energy, in BTU/bu, was consumed?

Step 1: Head (H) = PMPR (55/0.145\*0.102) + PMPD (200\*0.3048) = 99.6

Step 2: Pumping Energy (PPE) = (100 x 0.0979 x (8.6 x 25.4) x (225\*0.4) / (0.75 x 1 x 0.95 x 1)) x 948 BTU/MJ = 255,185,879 BTU/field

Step 3: Irrigation Energy (**IE**) = 255,185,879 /225

= 1,134,159 BTU/acre

|  |
| --- |
| **Required User Input Data:**  **Required conversion factors:** |
| Energy Source *(ES)*  PSI to meters/psi *(ME) = .703448* |
| Pump pressure *(PMPR)* via Table 7feet to meters *(FM) =.3048* |
| Pumping Depth *(PMDP)* via Table 8Inches to mm *(IM) = 25.4* |
| Annual irrigation water applied in acre-inches *(W)* Pump conversion factor *(PCF)*= .0979 |
| Fuel amount (in gallons) if known *(FA)* Acres to hectares (ATH) = .4 |
| Electricity amount (if known) (*EA)* Hectares to acres (HTA) = 2.47 |
| Irrigated Yield (*Yi)* BTU to MJ (BTM)= 948 |
| **Additional information needed:** |
| Area of field *(AF)* BTU/gal fuel *(BF)* = take from Table 1 . based on fuel type selected |
| BTU/kWh *(BK)* = take from Table 1 |
| On-Grid factor *(OGF)* = 3\* |
| Pump efficiency *(PE)=.75* |
| Irrigation efficiency (*IE)*= 1 |
| Gear head efficiency (*GHE)* = .95 |
| Power unit efficiency *(PUE)* = 1 |
| Conversion factor (C ) = 0.0979 (unitless) |
|  |
|  |
|  |

*\*=accounts for Production and transmission loss (FTM calculation from USDOE data)*

*Calculations based on equations 19.1, 19.2 and table 19.1 on pages 723&724 of: Hoffman, G.J., T.A. Howell, and K.H. Solomon. 1992. Management of Farm Irrigation Systems, ASAE Monograph Number 9.*

PROPOSED CHANGE: If electricity is selected as the energy source, ask the user “Is electricity generated on farm?” If the answer is “yes”, remove the on-grid factor (OGF) from the calculations below.

**Calculation:** Three options are described here, based on the type of information provided about fuel or electricity used to power the irrigation equipment.

**Option #1**: If fuel selected as energy source and fuel amount entered, then irrigation energy is calculated as the fuel amount (in BTU) divided by the area of the field:

Irrigation Energy (**IE**) = (FA x BF) / (AF) = BTU/acre

**IEy**= IE/*Yi*